For FMR:

1. We have to vary from 30mT to 90mT, and apply a 9 GHz signal from Signal Generator
2. At 69mT we should see a resonance